CS655 PA1

Xingkun Yin

U44255956

**Part 1**

Logistics:

The part one implement a very simple client and server app where server echo back the message it get from client.

Server:

To start the server, go to pa1part1 and type in

python server.py <port number>

You can pick any port number you like. I usually pick 58989. The server will create a socket that bind to that port number and ip address of 0.0.0.0 which would bind to all interface.